### Test 060-11-01 BUZ Command

Determine proper use of the BUZ command code 0x6A (Table 19) and the proper processing of the command by the PD with the appropriate sound.

##### PD

PD process BUZ command and makes an audible response that corresponds to the timing and frequency as specified in the BUZ command.

##### ACU

ACU MUST issue valid BUZ command and code values (Table 19).

#### Purpose

Used by ACU to generate an audible signal by the PD associated with a specified reader interaction.

#### Criteria

|  |  |
| --- | --- |
| Basic OSDP (PD) | Required |
| Basic OSDP (ACU) | Optional |
| Secure Channel (PD) | Required |
| Secure Channel (ACU) | Optional |
| BIO Match (PD) | Required |
| BIO Match (ACU) | Optional |
| BIO Read (PD) | Required |
| BIO Read (ACU) | Optional |
| Extended Packet Mode (PD) | Optional |
| Extended Packet Mode (ACU) | Optional |
| Extended Read/Write (PD) | Optional |
| Extended Read/Write (ACU) | Optional |

#### Test action

##### PD Test

When sent a BUZ the PD will make an audible sound corresponding to the BUZ command that is confirmed by observation on the part of the test engineer.

##### ACU Test

ACU sends osdp\_BUZ 0x6A command that is received and properly processed by the PD.

#### Development status

Available in libosdp-conformance [1.31-Build-4](https://github.com/Security-Industry-Association/libosdp-conformance/releases/tag/1.31-4)

#### Test Results

JSON tags

|  |  |
| --- | --- |
| test | 060-11-1 |
| test-status | 1 for pass, 0 for fail |

#### Revision History

New as 2.4.2