### Test 060-12-01 TEXT Command

Determine proper use of the TEXT command code 0x6B (Tables 20 and 21) and the proper processing of the command by the PD with the appropriate text output when this capability is reported by the PD.

##### PD

PD processes TEXT command and displays appropriate test in accordance with the TEXT command values (Table 21).

##### ACU

ACU MUST issue valid TEXT command and code values (Table 19).

#### Purpose

Used by ACU to generate a text display by the PD

#### Criteria

|  |  |
| --- | --- |
| Basic OSDP (PD) | Required |
| Basic OSDP (ACU) | Optional |
| Secure Channel (PD) | Required |
| Secure Channel (ACU) | Optional |
| BIO Match (PD) | Required |
| BIO Match (ACU) | Optional |
| BIO Read (PD) | Required |
| BIO Read (ACU) | Optional |
| Extended Packet Mode (PD) | Optional |
| Extended Packet Mode (ACU) | Optional |
| Extended Read/Write (PD) | Optional |
| Extended Read/Write (ACU) | Optional |

#### Test action

##### PD Test

When sent a TEXT command the PD process the command and provide the correct character display, if supported, and a NAK indicated the command is not supported. The test engineer observes the proper text display.

##### ACU Test

ACU sends osdp\_TEXT 0x6b command that is received and properly processed by the PD and observed by the test engineer.

#### Development status

Available in libosdp-conformance [1.31-Build-4](https://github.com/Security-Industry-Association/libosdp-conformance/releases/tag/1.31-4)

#### Test Results

JSON tags

|  |  |
| --- | --- |
| test | 060-12-1 |
| test-status | 1 for pass, 0 for fail |

#### Revision History

New as 2.4.2