### Test 060-21-01 Keep Reader Active KEEPACTIVE

##### This command instructs the PD to continue reader operations for the specified time limit to maintain communications with the credential.

##### PD

PD support of KEEPACTIVE 0xA7 command as described in Table 29.

##### ACU

ACU support of KEEPACTIVE 0xA7 command as described in Table 29.

#### Purpose

Used to support reader operations during card reads and other activities which may require extended processing times.

#### Criteria

|  |  |
| --- | --- |
| Basic OSDP (PD) | Optional |
| Basic OSDP (ACU) | Optional |
| Secure Channel (PD) | Optional |
| Secure Channel (ACU) | Optional |
| BIO Match (PD) | Optional |
| BIO Match (ACU) | Optional |
| BIO Read (PD) | Optional |
| BIO Read (ACU) | Optional |
| Extended Packet Mode (PD) | Required |
| Extended Packet Mode (ACU) | Required |
| Extended Read/Write (PD) | Optional |
| Extended Read/Write (ACU) | Optional |

#### Test action

##### PD Test

Test PD for support of KEEPACTIVE.

##### ACU Test

Test ACU for support of KEEPACTIVE.

.

#### Development status

Available in libosdp-conformance [1.31-Build-4](https://github.com/Security-Industry-Association/libosdp-conformance/releases/tag/1.31-4)

#### Test Results

JSON tags

|  |  |
| --- | --- |
| test | 060-21-01 |
| test-status | 1 for pass, 0 for fail |

#### Revision History

New as 2.4.2