### Test 060-23-01 Get PIV Data PIVDATA

##### Instructs PD to get PIV data contents of PIV card.

##### PD

PD support of PIVDATA 0xA3 command with data as described in Table 62 PIV Data Reply PIVDATAR.

##### ACU

ACU support of PIVDATA 0xA3 command with data as described in Table 31 and process PIV Data Reply.

#### Purpose

Support processing of PIV cards

#### Criteria

|  |  |
| --- | --- |
| Basic OSDP (PD) | Optional |
| Basic OSDP (ACU) | Optional |
| Secure Channel (PD) | Optional |
| Secure Channel (ACU) | Optional |
| BIO Match (PD) | Optional |
| BIO Match (ACU) | Optional |
| BIO Read (PD) | Optional |
| BIO Read (ACU) | Optional |
| Extended Packet Mode (PD) | Required |
| Extended Packet Mode (ACU) | Required |
| Extended Read/Write (PD) | Required |
| Extended Read/Write (ACU) | Required |

#### Test action

##### PD Test

The PD process the PIVDATA command and return PIVDATAR, determine this was done as described in Table 62.

##### ACU Test

Issue PIVDATA command and process PIVDATAR response as per Tables 31 and 62.

.

#### Development status

Available in libosdp-conformance [1.31-Build-4](https://github.com/Security-Industry-Association/libosdp-conformance/releases/tag/1.31-4)

#### Test Results

JSON tags

|  |  |
| --- | --- |
| test | 060-23-01 |
| test-status | 1 for pass, 0 for fail |

#### Revision History

New as 2.4.2