### Test 070-03-03 NAK Error Code 0 Should Fail

Determine PD does not NAK error code 00x0, if so fail.

##### PD

PD MUST NOT respond with NAK to 0x00

##### ACU

n/a

#### Purpose

Used to determine proper use of NAK by PD.

#### Criteria

|  |  |
| --- | --- |
| Basic OSDP (PD) | MUST NOT |
| Basic OSDP (ACU) | MUST NOT |
| Secure Channel (PD) | MUST NOT |
| Secure Channel (ACU) | MUST NOT |
| BIO Match (PD) | MUST NOT |
| BIO Match (ACU) | MUST NOT |
| BIO Read (PD) | MUST NOT |
| BIO Read (ACU) | MUST NOT |
| Extended Packet Mode (PD) | MUST NOT |
| Extended Packet Mode (ACU) | MUST NOT |
| Extended Read/Write (PD) | MUST NOT |
| Extended Read/Write (ACU) | MUST NOT |

#### Test action

##### PD Test

Monitor and determine PD does not NAK Error Code 00x0.

##### ACU Test

n/a

#### Development status

Available in libosdp-conformance [1.31-Build-4](https://github.com/Security-Industry-Association/libosdp-conformance/releases/tag/1.31-4)

#### Test Results

JSON tags

|  |  |
| --- | --- |
| test | 070-03-03 |
| test-status | 1 for pass, 0 for fail |

#### Revision History

New as 2.4.2