### Test 070-08-01 OSTATR Output Status Report

#### Description

##### PD

Provide change in output status in 0x4A response to osdp\_OSTAT 0x66 command if there is a change in output status monitored by the PD.

##### ACU

Accept this capability, and whether it is used.

#### Purpose

Determine ability to monitor status and changes of status of outputs of the PD.

#### Criteria

|  |  |
| --- | --- |
| Basic OSDP (PD) | Required |
| Basic OSDP (ACU) | Required |
| Secure Channel (PD) | Required |
| Secure Channel (ACU) | Required |
| BIO Match (PD) | Required |
| BIO Match (ACU) | Required |
| BIO Read (PD) | Required |
| BIO Read (ACU) | Required |
| Extended Packet Mode (PD) | Required |
| Extended Packet Mode (ACU) | Required |
| Extended Read/Write (PD) | Required |
| Extended Read/Write (ACU) | Required |

#### Test action

##### PD Test

Determine the output status capabilities reported and test output capabilities.

##### ACU Test

Support capabilities reported

#### Development status

Available in libosdp-conformance [1.31-Build-4](https://github.com/Security-Industry-Association/libosdp-conformance/releases/tag/1.31-4)

#### Test Results

JSON tags

|  |  |
| --- | --- |
| test | 070-08-01 |
| test-status | 1 for pass, 0 for fail |

#### Revision History

New for 2.4.2