### Test 070-18-01 MFGREP

#### Description

##### PD

Provide optional manufacturer specific reply 0x90 (Table 60) to manufacturer specific command or as a poll response.

##### ACU

Provide optional manufacturer specific command and process reply

#### Purpose

Allow manufacturer specific commands to be embedded in the protocol.

|  |  |
| --- | --- |
| Basic OSDP (PD) | Optional |
| Basic OSDP (ACU) | Optional |
| Secure Channel (PD) | Optional |
| Secure Channel (ACU) | Optional |
| BIO Match (PD) | Optional |
| BIO Match (ACU) | Optional |
| BIO Read (PD) | Optional |
| BIO Read (ACU) | Optional |
| Extended Packet Mode (PD) | Optional |
| Extended Packet Mode (ACU) | Optional |
| Extended Read/Write (PD) | Optional |
| Extended Read/Write (ACU) | Optional |

#### Test action

##### PD Test

Provide optional manufacturer specific reply 0x90 (Table 60) to manufacturer specific command or as a poll response for those supported for the device under test and as necessary to support testing.

##### ACU Test

Provide and process MFG command and MFGREP response

#### Development status

Available in libosdp-conformance [1.31-Build-4](https://github.com/Security-Industry-Association/libosdp-conformance/releases/tag/1.31-4)

#### Test Results

JSON tags

|  |  |
| --- | --- |
| test | 070-18-01 |
| test-status | 1 for pass, 0 for fail |

#### Revision History

New for 2.4.2

**+**