### Test 070-25-04 FSTAT Idle

#### Description

##### PD

##### Provide period of idle (FtDelay and FtStatusDetail) as described in section 7.25 in Table 67 as part of FTSTAT response.

##### ACU

Support file transfer capabilities reported, and idle as reported in FTSTAT and FtDelay and FtStatusDetail.

#### Purpose

Provide delays (idle) necessary for FILETRANSFER processing.

|  |  |
| --- | --- |
| Basic OSDP (PD) | Optional |
| Basic OSDP (ACU) | Optional |
| Secure Channel (PD) | Optional |
| Secure Channel (ACU) | Optional |
| BIO Match (PD) | Optional |
| BIO Match (ACU) | Optional |
| BIO Read (PD) | Optional |
| BIO Read (ACU) | Optional |
| Extended Packet Mode (PD) | Optional |
| Extended Packet Mode (ACU) | Optional |
| Extended Read/Write (PD) | Optional |
| Extended Read/Write (ACU) | Optional |

#### Test action

##### PD Test

Determine the PD provides proper idle response to FILETRANSFER as shown in Table 67.

##### ACU Test

Initiate and support FILETRANSFER and properly process FSTAT including idle.

#### Development status

Available in libosdp-conformance [1.31-Build-4](https://github.com/Security-Industry-Association/libosdp-conformance/releases/tag/1.31-4)

#### Test Results

JSON tags

|  |  |
| --- | --- |
| test | 070-25-04 |
| test-status | 1 for pass, 0 for fail |

#### Revision History

New for 2.4.2