### Test 060-19-01 Manufacturer Specific Command(s) MFG

##### This command is intended to allow manufacturer specific commands to be embedded within this protocol.

##### PD

Optional PD support of MFG command as described in Table 27.

##### ACU

Optional ACU support of MFG command as described in Table 27.

#### Purpose

Used to support manufacturer specific features.

#### Criteria

|  |  |
| --- | --- |
| Basic OSDP (PD) | Optional |
| Basic OSDP (ACU) | Optional |
| Secure Channel (PD) | Optional |
| Secure Channel (ACU) | Optional |
| BIO Match (PD) | Optional |
| BIO Match (ACU) | Optional |
| BIO Read (PD) | Optional |
| BIO Read (ACU) | Optional |
| Extended Packet Mode (PD) | Optional |
| Extended Packet Mode (ACU) | Optional |
| Extended Read/Write (PD) | Optional |
| Extended Read/Write (ACU) | Optional |

#### Test action

##### PD Test

Optionally test PD for support of manufacturer specific features.

##### ACU Test

Optionally test ACU for support of manufacturer specific features.

#### Development status

Available in libosdp-conformance [1.31-Build-4](https://github.com/Security-Industry-Association/libosdp-conformance/releases/tag/1.31-4)

#### Test Results

JSON tags

|  |  |
| --- | --- |
| test | 060-19-01 |
| test-status | 1 for pass, 0 for fail |

#### Revision History

New as 2.4.2