### Test 070-14-01 BIOREADR Scan and Send Biometric Data

#### Description

##### PD

Provide capability to scan and send biometric data when capability is reported in response to 0x57 osdp\_BIOREADR as in Table 58.

##### ACU

Process biometric data received in response to 0x57 osdp\_BIOREADR

#### Purpose

Support BIO Read profile scan, and send of BIOREADR data.

|  |  |
| --- | --- |
| Basic OSDP (PD) | Optional |
| Basic OSDP (ACU) | Optional |
| Secure Channel (PD) | Optional |
| Secure Channel (ACU) | Optional |
| BIO Match (PD) | Optional |
| BIO Match (ACU) | Optional |
| BIO Read (PD) | Required |
| BIO Read (ACU) | Required |
| Extended Packet Mode (PD) | Optional |
| Extended Packet Mode (ACU) | Optional |
| Extended Read/Write (PD) | Optional |
| Extended Read/Write (ACU) | Optional |

#### Test action

##### PD Test

Provide biometrics data as indicated in data section of Table 58.

##### ACU Test

Process biometric data in support of BIO Read profile

#### Development status

Available in libosdp-conformance [1.31-Build-4](https://github.com/Security-Industry-Association/libosdp-conformance/releases/tag/1.31-4)

#### Test Results

JSON tags

|  |  |
| --- | --- |
| test | 070-14-01 |
| test-status | 1 for pass, 0 for fail |

#### Revision History

New for 2.4.2