### Test 070-19-01 BUSY PD Busy Reply

#### Description

##### PD

Provide a BUSY 0x79 response to an osdp command if the PD is busy processing the previous command

##### ACU

Process BUSY response and maintain synchronization.

#### Purpose

Allow PD to complete processing of a command and let the ACU know this and maintain synchronization.

|  |  |
| --- | --- |
| Basic OSDP (PD) | Optional |
| Basic OSDP (ACU) | Optional |
| Secure Channel (PD) | Optional |
| Secure Channel (ACU) | Optional |
| BIO Match (PD) | Optional |
| BIO Match (ACU) | Optional |
| BIO Read (PD) | Optional |
| BIO Read (ACU) | Optional |
| Extended Packet Mode (PD) | Optional |
| Extended Packet Mode (ACU) | Optional |
| Extended Read/Write (PD) | Optional |
| Extended Read/Write (ACU) | Optional |

#### Test action

##### PD Test

Determine whether PD supports the optional BUSY feature, and if so induce BUSY and determine that synchronization with the ACU in maintain.

##### ACU Test

Process optional BUSY and maintain synchronization.

#### Development status

Available in libosdp-conformance [1.31-Build-4](https://github.com/Security-Industry-Association/libosdp-conformance/releases/tag/1.31-4)

#### Test Results

JSON tags

|  |  |
| --- | --- |
| test | 070-19-01 |
| test-status | 1 for pass, 0 for fail |

#### Revision History

New for 2.4.2